# Summary

* [Glossary](gloss.md)
* [Clever 2 assembly](assemble_2.md)
* [Clever 3 assembly](assemble_3.md)
* [Connecting 4 in 1 ESCs](4in1.md)
* [Types of power connectors](connectortypes.md)
* [Blanching](zap.md)
* [Initial setup](setup.md)
* [Using multimeter](test_connection.md)
* [Possible radio failures](radioerrors.md)
* [Installation of FPV](fpv.md)
* [Safety instruction](safety.md)
* [Soldering safety](tb.md)
* [Connecting GPS](gps.md)
* [Flight modes](modes.md)
* [Pixhawk / Pixracer Firmware](firmware.md)
* [PX4 Parameters](px4_parameters.md)
* [PID Setup](calibratePID.md)
* [Raspberry Pi](raspberry.md)
* [RPi Image](microsd_images.md)
* [RPi Connection to the Pixhawk](connection.md)
* [Wi-Fi connection](wifi.md)
* [Configuring Wi-Fi](network.md)
* [Using QGroundControl via Wi-Fi](gcs_bridge.md)
* [Controlling Clever from a smartphone](rc.md)
* [UART settings](uart.md)
* [Viewing images from cameras](web_video_server.md)
* [Coordinate systems (frames)](frames.md)
* [ROS](ros.md)
* [MAVROS](mavros.md)
* [Simple OFFBOARD](simple_offboard.md)
* [Navigation using ArUco markers](aruco.md)
* [Automatic check](selfcheck.md)
* [Code examples](snippets.md)
* [Adjusting the position of the main camera](camera_frame.md)
* [Working with the camera](camera.md)
* [Working with a LED strip on Raspberry 3](leds.md)
* [Using rviz and rqt](rviz.md)
* [Working with the ultrasonic distance gage](sonar.md)
